Stereo Connectors - Pre-Facelift Mk3
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Note: This wiring information does not cover pre-facelift Navigation Systems, although some of the information may still be relevant/correct 

The following figures illustrate the basic connector layouts and give pin numbers which correspond to the lists below. 
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· 1 Connector A (C483) 

· 1.1 Power (with RSE = C489) 

· 2 Connector B (C484) 

· 2.1 Speakers 

· 3 Connector C (C485) 

· 3.1 Data 


Connector A (C483)
Power (with RSE = C489)
Pin 1 (Orange/Black) Battery + (From Fuse F72) (20A) 

Pin 2 (Black/Yellow) Keycode Ground 

Pin 3 (Blue/Black) Ign. Sense (Accessory) (From Fuse F69) (7.5A) 

Pin 4 (Orange/Black) Illumination 

Pin 5 (Black/Orange) Alarm Sense (From GEM) 

Pin 6 (Black/Green) Ground 

Pin 7 (Orange/Green) Not Used on C483 / To multimedia control module on cars with Rear Seat Videos (C489) / To telematics module on cars with phone prep (C1003) 

Connector B (C484)
Speakers
Pin 1 (White/Black) Left Front – 

Pin 2 (Grey/Black) Left Front + 

Pin 3 (White/Violet) Left Rear – 

Pin 4 (Grey/White) Left Rear + 

Pin 5 (White/Red) Right Front – 

Pin 6 (Grey/Red) Right Front + 

Pin 7 (White/Right) Rear – 

Pin 8 (Grey/Right) Rear + 

Connector C (C485)
Data
Pin 1 (Grey/Black) Telematics 

Pin 2 (Blue/Yellow) Telematics 

Pin 3 Not Used 

Pin 4 (Black/Red) Telematics - When fitting Handsfree phone kits, this is where the stereo mute wire goes 

Pin 5 (White) Telematics 

Pin 6 (White/Green) VSS 

Pin 7 Not Used 

Pin 8 (White/Red) Telematics 

Pin 9 (White/Red) Telematics 

Pin 10 (Green/White) Reverse Sense (For Navigation) 

Pin 11 (White/Black) Steering Column Remote Stalk 

Pin 12 (Brown/Yellow) Steering Column Remote Stalk 

Pin 13 Not Used 

Pin 14 Not Used 

Pin 15 Not Used 

Pin 16 (White/Green) Data Link Connector 

Pin 17 (Black/Green) Restraints Control Module / Telematics
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